

Experiment – 8


**Configure the Dynamic NAT using cisco packet tracer.**


1. Initial Connection




1. Configuration









1. Final Output

