
Module – 5

NS2 Simulator


**Experiment – 01**

**Four Node Point to Point Network**


TCL file :


****


AWK file: -




**OUTPUT**

****

****


****


****


**Experiment – 2**

**Transmission of Ping Message**


**TCL File: -**

****

****


****


**AWK File: -**

****

**OUTPUT**


**TCL**

****

****

**AWK**


****


****


**Experiment – 3**

**Ethernet LAN using N-Nodes**


**TCL File: -**

****

****


****


**AWK File: -**

****


**OUTPUT**

**TCL**


****

****

**AWK**

****


**Simulation:**




**Experiment – 4**


**Simple ESS With Wireless LAN**

**TCL File: -**

****


****


**AWK File: -**

****


**OUTPUT**

**TCL**


****

****

**AWK**

****

**Simulation**

****

**Simulation:**

